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Compound gas detection transmitter

产品介绍：      
复合式气体检测变送器采用非标协议或MODBUS协议进行数据采集和传输，可以最多同时检测四种气体，全中文显示，操作简单。可以按键操作或者使用遥控器设置参数。
智能变送器节点对现场的气体浓度进行采集检测，主机轮巡检测各个节点，配合智能化的后
台软件，实时监控现场气体浓度变化。抗干扰能力强，布局方便，接线简单，同时智能变送器节点还提供一个无源开关量输出，可控制外部设备。
检测仪以自然扩散的方式检测气体浓度，采用进口传感器，具有良好的灵敏度和出色的重复
性；仪器采用嵌入式微控技术，可靠性高。
检测仪外壳采用铸铝材料，强度高，耐温，耐腐蚀。本产品适用于检测环境空气中有毒
有害、易燃易爆气体的浓度，广泛使用于冶金、电厂、化工、矿井、隧道、坑道、地下管线
等场所，有效的预防事故的发生。
The compound gas detection transmitter adopts non-standard agreement or MOdBUS protocol for data collection and transmission,it can detect 4 kind of gases. With chinese display,simple key buttons operation and remote control to set up parameters.
The intelligent transmitter node acquisition collects and detects the gas concentration at the leak point. The host round tests various nodes with intelligent background software, and monitoring the gas concentration changes in real-time. Our product uses the bus-system, having strong anti-jamming capability, convenient layout and simple wiring. At the same time, it also provides an controlling external device (exhaust fan, solenoid valve, etc.) of the switch output.
The detector detects gas concentration with natural diffusion mode, which uses the imported sensors and has a good sensitivity and repeatability.
This instrument uses the embedded micro-controller control technology, simple menu operation, complete functions and high reliability. Bus-system gas detection transmitter adopts aluminum shell material with high strength, heat resistance and corrosion resistance. Our product is suitable for the detection of poisonous and harmful, inflammable and explosive gas in the air and has been widely used in metallurgy, power plant, chemical industry, mine, tunnel, tunnels, underground pipeline and other places, effectively preventing the happening of the accident.


基本参数：
外形尺寸：142mm×178.5mm×91mm
重    量：约1.35kg
传感器类型：电化学式（可燃气为催化燃烧式，特殊的另行说明）
检测气体：氧气（O2）、可燃气（EX）、有毒有害气体
                （CO、H2S、NH3、CL2等）
响应时间：氧气≤30s；一氧化碳≤40s；可燃气≤20s；（其它略）
工作模式：连续工作
工作电压：DC12V~36V 
输出信号：RS485\二总线\433MHz
显示方式：图形液晶显示
控制信号：无源开关量输出，最大负荷250V AC 3A
附加功能：时间、日历显示，可存储3000+条数据记录
温度范围：-20℃～50℃
湿度范围：15%～90%（RH）无冷凝
防爆证号：CE10 1084
防爆标志：Exd II CT6
接线方式：RS485为四线制接线方式，二总线为两线，433MHz为两线。
传输电缆：屏蔽电缆 RVVP1.0
传输距离：小于1000m
Basic parameters:
Size：142mm * 178.5 mm * 91 mm
Weight: about 1350 g
Sensor types: electrochemistry method
(gas catalytic combustion type, special separately)
Destination gas: oxygen (O2), gas (EX), 
poisonous and harmful gases (CO, H2S, NH3, CL2, etc.)
Response time: ≤30s(O2);≤40s(CO);≤20s(EX)
Working pattern: continuous work
Working voltage: DC24V
Output signal: 485 digital signal/two bus wire/433MHz
Display: Graph LCD Module
Control signal: Switch output, the maximum load 250 V AC 3A
Additional features: time, calendar display,can keep 3000+records



Temperature range: - 20 ℃ ~ 50 ℃
Humidity:  15% ~ 90% RH (No condensation)
Explosion-proof number: CE10 1084
Explosion-proof marks: Exd II CT6
Connection mode: RS485 is four wire connection mode,Two bus wire is two wire; 433MHz is two wire
Transmission cables: Shield cable RVVP1.0
Transmission distance: ＜ 1000 m

